Table 1: Flood Hazard Maps, Flood Risk Maps and Total damage corresponding to each water level at Can Tho gauging station

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No** | **Water level  (m)** | **Flood Hazard map** | **Flood Risk Map** | **Total damage  (million USD)** |
|
| 1 | 1.82 | HAZARD\_MAP\_1.82m | RISK\_MAP\_1.82m | 2.53 |
| 2 | 2.04 | HAZARD\_MAP\_2.04m | RISK\_MAP\_2.04m | 5.30 |
| 3 | 2.15 | HAZARD\_MAP\_2.15m | RISK\_MAP\_2.15m | 12.97 |
| 4 | 2.18 | HAZARD\_MAP\_2.18m | RISK\_MAP\_2.18m | 15.39 |
| 5 | 2.69 | HAZARD\_MAP\_2.69m | RISK\_MAP\_2.69m | 71.99 |
| 6 | 2.72 | HAZARD\_MAP\_2.72m | RISK\_MAP\_2.72m | 74.18 |